# Fusion-Wild-Bar 0.1.7-rc Public Release Infos

Firmware Release 0.1.7-rc from 2026-02-12.

Built from the following components:

- Fixtures/Fusion-Wild-Bar/Main: 0.1.7-rc
- Drivers/impression-X5/LED-Driver: 0.15.7
- Drivers/Universal/Fan-Driver-G0: 0.5.0
- Drivers/Universal/Motor-Driver: 0.8.2
- Drivers/Universal/Network-Interface: 0.4.5
- Drivers/Universal/DIC: 0.1.5

## Warnings

- A CRITICAL BUG WAS FIXED IN BOOTLOADER 2.2.1! Make sure all driver bootloaders are updated to version 2.2.1 before attempting any update. If this is not obeyed, the Network Interface can be bricked and requires opening of the fixture!

## Not Implemented

- Service Mode
- Fixture-to-Fixture Firmware Push

## Release Changes

Internal maintenance release.

## Previous Version [0.1.6-rc] - 2026-02-11

### Fixed

- FX Tungsten indices are now as specified in the DMX chart. They were previously offset by -10.

## Previous Version [0.1.5-rc] - 2025-12-19

Internal maintenance release.

## Previous Version [0.1.4-rc.1] - 2025-03-31

### Fixed

- Fixed incorrect 'CRMX: Module not Responding' error message when using CRMX

## Previous Version [0.1.3-rc] - 2025-03-12

Internal maintenance release.

## Previous Version [0.1.2-rc.5] - 2024-12-13

Internal maintenance release.

## Previous Version [0.1.1-rc.5] - 2024-09-25

Internal maintenance release.